<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="3.683" y1="20.193" x2="31.242" y2="20.193" width="0" layer="20"/>
<wire x1="31.242" y1="20.701" x2="31.242" y2="34.798" width="0" layer="20"/>
<wire x1="31.242" y1="34.798" x2="31.242" y2="35.306" width="0" layer="20"/>
<wire x1="31.242" y1="35.306" x2="3.683" y2="35.306" width="0" layer="20"/>
<wire x1="3.683" y1="35.306" x2="3.683" y2="34.798" width="0" layer="20"/>
<wire x1="3.683" y1="34.798" x2="3.683" y2="20.701" width="0" layer="20"/>
<wire x1="3.683" y1="20.701" x2="3.683" y2="20.193" width="0" layer="20"/>
<wire x1="3.683" y1="34.798" x2="31.242" y2="34.798" width="0" layer="46"/>
<wire x1="31.242" y1="34.798" x2="31.242" y2="20.701" width="0" layer="46"/>
<wire x1="31.242" y1="20.701" x2="3.683" y2="20.701" width="0" layer="46"/>
<wire x1="3.683" y1="20.701" x2="3.683" y2="34.798" width="0" layer="46"/>
<wire x1="31.242" y1="34.798" x2="3.683" y2="34.798" width="0" layer="20"/>
<wire x1="3.683" y1="20.701" x2="31.242" y2="20.701" width="0" layer="20"/>
<wire x1="31.242" y1="20.193" x2="31.242" y2="20.701" width="0" layer="20"/>
<text>Core</text>
<text>v3</text>
<text>Mod</text>
<text>www.auml.se</text>
<text>Component layout</text>
<text>Copper, top side</text>
<text>Copper, bottom side</text>
<text>Silcscreen, top side</text>
<text>Soldermask, top side</text>
<text>Soldermask, bottom side</text>
<text>This work by http://projekt.auml.se is licensed under a</text>
<text>Creative Commons Attribution-Share Alike 3.0 Unported License</text>
<text>http://creativecommons.org/licenses/by-sa/3.0/</text>
<text>Cut border</text>
</plain>
<libraries>
<library name="mcp2551">
<packages>
<package name="SOIC">
</package>
</packages>
</library>
<library name="mcp2515">
<packages>
<package name="TSSOP">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
</package>
<package name="R0402">
</package>
<package name="C1210">
</package>
<package name="L1210">
</package>
<package name="C0805">
</package>
</packages>
</library>
<library name="avrisp">
<packages>
<package name="6PINSMD">
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO-220AA">
</package>
</packages>
</library>
<library name="atmega88">
<packages>
<package name="MLF32">
</package>
</packages>
</library>
<library name="expboard">
<packages>
<package name="CORETWO_PIN">
</package>
</packages>
</library>
<library name="pinhead-mm">
<packages>
<package name="1X01_SMD">
</package>
</packages>
</library>
<library name="xtal_CSTCE">
<packages>
<package name="SMD">
</package>
</packages>
</library>
<library name="tc1047a">
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="BD9G101G">
<packages>
<package name="SSOP6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="mcp2551" package="SOIC" value="MCP2551">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="mcp2515" package="TSSOP" value="MCP2515">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="avrisp" package="6PINSMD" value="AVRISP6PIN">
<attribute name="VALUE"/>
</element>
<element name="R50" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L1210" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="C0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="C1210" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO-220AA" value="">
<attribute name="NAME"/>
</element>
<element name="C20" library="rcl" package="C0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="atmega88" package="MLF32" value="ATMEGA88-M32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="VCC" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="V_CAN" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_A" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_B" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_C" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_D" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_E" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_F" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_G" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_H" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_I" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_J" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_K" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_L" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_M" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_N" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_O" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_P" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_Q" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="EXP_R" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="CANL" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="CANH" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="JP1" library="pinhead-mm" package="1X01_SMD" value=""/>
<element name="JP3" library="pinhead-mm" package="1X01_SMD" value=""/>
<element name="JP2" library="pinhead-mm" package="1X01_SMD" value=""/>
<element name="JP4" library="pinhead-mm" package="1X01_SMD" value=""/>
<element name="Q1" library="xtal_CSTCE" package="SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="tc1047a" package="SOT23" value="TC1047A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCK" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="MISO" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="RST" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="MOSI" library="expboard" package="CORETWO_PIN" value="CORETWO_PIN"/>
<element name="IC5" library="BD9G101G" package="SSOP6" value="BD9G101G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="X2" pad="6"/>
<contactref element="R51" pad="1"/>
<contactref element="C43" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="C20" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="21"/>
<contactref element="IC3" pad="BPAD"/>
<contactref element="GND" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="R53" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="20"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="X2" pad="2"/>
<contactref element="IC1" pad="19"/>
<contactref element="L1" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="18"/>
<contactref element="VCC" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="R52" pad="2"/>
<contactref element="C42" pad="1"/>
<contactref element="R40" pad="2"/>
<contactref element="C44" pad="2"/>
</signal>
<signal name="V_CAN">
<contactref element="C41" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="V_CAN" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="CANH">
<contactref element="IC2" pad="7"/>
<contactref element="CANH" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="INT">
<contactref element="IC1" pad="13"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="14"/>
<contactref element="X2" pad="3"/>
<contactref element="IC3" pad="17"/>
<contactref element="SCK" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="16"/>
<contactref element="X2" pad="4"/>
<contactref element="IC3" pad="15"/>
<contactref element="MOSI" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="17"/>
<contactref element="X2" pad="1"/>
<contactref element="IC3" pad="16"/>
<contactref element="MISO" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="IC1" pad="3"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="CS">
<contactref element="IC1" pad="18"/>
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="26"/>
</signal>
<signal name="CANL">
<contactref element="IC2" pad="6"/>
<contactref element="CANL" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="X2" pad="5"/>
<contactref element="IC3" pad="29"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="RXCAN">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="TXCAN">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="OSC1">
<contactref element="IC1" pad="9"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="OSC2">
<contactref element="IC1" pad="8"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="V_CAN-FEEDBACK">
<contactref element="R50" pad="1"/>
<contactref element="R51" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="CB">
<contactref element="C40" pad="1"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="VSW">
<contactref element="L1" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="EXP_R">
<contactref element="IC3" pad="20"/>
<contactref element="EXP_R" pad="1"/>
</signal>
<signal name="EXP_B">
<contactref element="IC3" pad="14"/>
<contactref element="EXP_B" pad="1"/>
</signal>
<signal name="EXP_A">
<contactref element="IC3" pad="8"/>
<contactref element="EXP_A" pad="1"/>
</signal>
<signal name="EXP_C">
<contactref element="IC3" pad="13"/>
<contactref element="EXP_C" pad="1"/>
</signal>
<signal name="EXP_D">
<contactref element="IC3" pad="12"/>
<contactref element="EXP_D" pad="1"/>
</signal>
<signal name="EXP_E">
<contactref element="IC3" pad="11"/>
<contactref element="EXP_E" pad="1"/>
</signal>
<signal name="EXP_F">
<contactref element="IC3" pad="10"/>
<contactref element="EXP_F" pad="1"/>
</signal>
<signal name="EXP_G">
<contactref element="IC3" pad="9"/>
<contactref element="EXP_G" pad="1"/>
</signal>
<signal name="EXP_H">
<contactref element="IC3" pad="2"/>
<contactref element="EXP_H" pad="1"/>
</signal>
<signal name="EXP_I">
<contactref element="IC3" pad="32"/>
<contactref element="EXP_I" pad="1"/>
</signal>
<signal name="EXP_J">
<contactref element="IC3" pad="31"/>
<contactref element="EXP_J" pad="1"/>
</signal>
<signal name="EXP_K">
<contactref element="IC3" pad="30"/>
<contactref element="EXP_K" pad="1"/>
</signal>
<signal name="EXP_L">
<contactref element="IC3" pad="28"/>
<contactref element="EXP_L" pad="1"/>
</signal>
<signal name="EXP_M">
<contactref element="IC3" pad="27"/>
<contactref element="EXP_M" pad="1"/>
</signal>
<signal name="EXP_N">
<contactref element="IC3" pad="25"/>
<contactref element="EXP_N" pad="1"/>
</signal>
<signal name="EXP_O">
<contactref element="IC3" pad="24"/>
<contactref element="EXP_O" pad="1"/>
</signal>
<signal name="EXP_P">
<contactref element="IC3" pad="23"/>
<contactref element="EXP_P" pad="1"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="EXP_Q">
<contactref element="IC3" pad="22"/>
<contactref element="EXP_Q" pad="1"/>
</signal>
<signal name="CAN_RS">
<contactref element="IC2" pad="8"/>
<contactref element="R53" pad="2"/>
<contactref element="R52" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="R41" pad="2"/>
<contactref element="R40" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="C44" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
